---
title: "Mi configuracion impresion 3d slic3r overload pro+ dreammaker"
date: 2023-06-14T21:10:46-03:00
tags: ['slic3r','configuracion','impresion','3d','dreammaker']
---

Este es el archivo de configuración de slic3r que uso para hacer impresiones 3d con el modelo de impresora DreamMaker Overload Pro+

Caracteristicas de esta impresora:  
[Ficha-Impresora-3D.pdf](/files/Ficha-Impresora-3D.pdf)

Mi configuracion actual, todavia no es optima.
```console
# generated by Slic3r 1.3.0 on Wed Jun 14 23:21:15 2023

[filament:1.75mm Filamento OverloadPro]
bed_temperature = 60
bridge_fan_speed = 100
compatible_printers = 
cooling = 1
disable_fan_first_layers = 3
end_filament_gcode = "; Filament-specific end gcode \n;END gcode for filament\n"
extrusion_multiplier = 1
fan_always_on = 0
fan_below_layer_time = 60
filament_colour = #000000
filament_cost = 0
filament_density = 0
filament_diameter = 1.75
filament_max_volumetric_speed = 0
filament_notes = ""
filament_settings_id = 
first_layer_bed_temperature = 65
first_layer_temperature = 210
max_fan_speed = 100
min_fan_speed = 35
min_print_speed = 10
slowdown_below_layer_time = 5
start_filament_gcode = "; Filament gcode\n"
temperature = 198

[filament:My Settings]
bed_temperature = 60
bridge_fan_speed = 100
compatible_printers = 
cooling = 1
disable_fan_first_layers = 3
end_filament_gcode = "; Filament-specific end gcode \n;END gcode for filament\n"
extrusion_multiplier = 1
fan_always_on = 0
fan_below_layer_time = 60
filament_colour = #FFFFFF
filament_cost = 0
filament_density = 0
filament_diameter = 1.75
filament_max_volumetric_speed = 0
filament_notes = ""
filament_settings_id = 
first_layer_bed_temperature = 65
first_layer_temperature = 205
max_fan_speed = 100
min_fan_speed = 35
min_print_speed = 10
slowdown_below_layer_time = 5
start_filament_gcode = "; Filament gcode\n"
temperature = 200

[presets]
filament = 1.75mm Filamento OverloadPro
print = My Settings
printer = My Settings

[print:My Settings]
adaptive_slicing = 0
adaptive_slicing_quality = 75%
avoid_crossing_perimeters = 0
bottom_infill_pattern = rectilinear
bottom_solid_layers = 3
bridge_acceleration = 0
bridge_flow_ratio = 1
bridge_speed = 20
brim_connections_width = 0
brim_width = 5
compatible_printers = 
complete_objects = 0
default_acceleration = 0
dont_support_bridges = 1
external_perimeter_extrusion_width = 0
external_perimeter_speed = 50%
external_perimeters_first = 0
extra_perimeters = 1
extruder_clearance_height = 20
extruder_clearance_radius = 20
extrusion_width = 0
fill_angle = 45
fill_density = 20%
fill_gaps = 0
fill_pattern = rectilinear
first_layer_acceleration = 0
first_layer_extrusion_width = 200%
first_layer_height = 0.3
first_layer_speed = 30%
gap_fill_speed = 20
gcode_comments = 0
infill_acceleration = 0
infill_every_layers = 1
infill_extruder = 1
infill_extrusion_width = 0
infill_first = 0
infill_only_where_needed = 0
infill_overlap = 55%
infill_speed = 80
interface_shells = 0
interior_brim_width = 0
layer_height = 0.2
match_horizontal_surfaces = 0
max_print_speed = 80
max_volumetric_speed = 0
min_skirt_length = 0
notes = 
only_retract_when_crossing_perimeters = 1
ooze_prevention = 0
output_filename_format = [input_filename_base].gcode
overhangs = 1
perimeter_acceleration = 0
perimeter_extruder = 1
perimeter_extrusion_width = 0
perimeter_speed = 60
perimeters = 3
post_process = 
print_settings_id = 
raft_layers = 0
regions_overlap = 0
resolution = 0
seam_position = aligned
shortcuts = support_material
skirt_distance = 6
skirt_height = 1
skirts = 1
small_perimeter_speed = 15
solid_infill_below_area = 70
solid_infill_every_layers = 0
solid_infill_extruder = 1
solid_infill_extrusion_width = 0
solid_infill_speed = 20
spiral_vase = 0
standby_temperature_delta = -5
support_material = 0
support_material_angle = 0
support_material_buildplate_only = 0
support_material_contact_distance = 0.2
support_material_enforce_layers = 0
support_material_extruder = 1
support_material_extrusion_width = 0
support_material_interface_extruder = 1
support_material_interface_extrusion_width = 0
support_material_interface_layers = 3
support_material_interface_spacing = 0
support_material_interface_speed = 100%
support_material_max_layers = 0
support_material_pattern = rectilinear
support_material_spacing = 5
support_material_speed = 20
support_material_threshold = 60%
thin_walls = 1
top_infill_extrusion_width = 0
top_infill_pattern = rectilinear
top_solid_infill_speed = 15
top_solid_layers = 3
travel_speed = 90
xy_size_compensation = 0

[printer:My Settings]
bed_shape = 99.4522x10.4528,97.8148x20.7912,95.1057x30.9017,91.3545x40.6737,86.6025x50,80.9017x58.7785,74.3145x66.9131,66.9131x74.3145,58.7785x80.9017,50x86.6025,40.6737x91.3545,30.9017x95.1057,20.7912x97.8148,10.4528x99.4522,0x100,-10.4528x99.4522,-20.7912x97.8148,-30.9017x95.1057,-40.6737x91.3545,-50x86.6025,-58.7785x80.9017,-66.9131x74.3145,-74.3145x66.9131,-80.9017x58.7785,-86.6025x50,-91.3545x40.6737,-95.1057x30.9017,-97.8148x20.7912,-99.4522x10.4528,-100x0,-99.4522x-10.4528,-97.8148x-20.7912,-95.1057x-30.9017,-91.3545x-40.6737,-86.6025x-50,-80.9017x-58.7785,-74.3145x-66.9131,-66.9131x-74.3145,-58.7785x-80.9017,-50x-86.6025,-40.6737x-91.3545,-30.9017x-95.1057,-20.7912x-97.8148,-10.4528x-99.4522,0x-100,10.4528x-99.4522,20.7912x-97.8148,30.9017x-95.1057,40.6737x-91.3545,50x-86.6025,58.7785x-80.9017,66.9131x-74.3145,74.3145x-66.9131,80.9017x-58.7785,86.6025x-50,91.3545x-40.6737,95.1057x-30.9017,97.8148x-20.7912,99.4522x-10.4528,100x0
before_layer_gcode = 
between_objects_gcode = 
end_gcode = M104 S0 ; turn off temperature\nG28 X0  ; home X axis\nM84     ; disable motors\n
extruder_offset = 0x0
gcode_flavor = reprap
has_heatbed = 1
host_type = octoprint
layer_gcode = 
max_layer_height = 0.3
min_layer_height = 0.15
nozzle_diameter = 0.4
octoprint_apikey = 
pressure_advance = 0
print_host = 
printer_notes = 
printer_settings_id = 
retract_before_travel = 2
retract_layer_change = 1
retract_length = 5
retract_length_toolchange = 10
retract_lift = 0
retract_lift_above = 0
retract_lift_below = 0
retract_restart_extra = 0
retract_restart_extra_toolchange = 0
retract_speed = 80
serial_port = 
serial_speed = 250000
start_gcode = G28 ; home all axes\nG1 Z5 F5000 ; lift nozzle\n
toolchange_gcode = 
use_firmware_retraction = 0
use_relative_e_distances = 0
use_set_and_wait_bed = 0
use_set_and_wait_extruder = 0
use_volumetric_e = 0
vibration_limit = 0
wipe = 1
z_offset = 0
z_steps_per_mm = 0

[settings]
autocenter = 1

```

