---
title: "X86 opcode"
date: 2024-09-07T03:08:00-03:00
tags: ['reversing']
---
'%' significa "and EAX"

'-' significa "sub EAX"

'P' significa "push EAX"

'X' significa "pop EAX"

'T' significa "push ESP"

'\' significa "pop ESP"


https://stackoverflow.com/questions/14349735/why-register-eax-esp-and-instructions-sub-push-and-pop-assemble-into-ascii-cha

http://ref.x86asm.net/coder32.html

